**Notes on BCR**

This BCR (Battery Charge Regulator) uses MPPT (Maximum Power Point Transfer) to control the charge current fed to the battery.

The MPPT is controlled by a number 12FC671 PIC microcontrollers.

The programming code for these PICs is no longer available.